

**EcoAqua AP2-C401-SG (Mini Lincat) Compatible Cartridge**

Code: EWF8002A

Fits the following filters:

3M® AP2-C401-SG, LINCAT® FC02

**Operating Specifications:**

Minimum operating temperature 0.6°C/33°F

Maximum operating temperature 38°C/100°F

Min. working pressure 140 kPa/20 psi

Max. working pressure 827 kPa/120 psi

Rated capacity 4,000 litres/1,060 gallons

Flow rate 1.9 lpm/0.5 gpm





*Distributed by:*

**Aqua Cure Ltd,**

**Aqua Cure House, Hall Street,**

**Southport, PR9 0SE.**

**Tel: 01704 516916**

[**www.aquacure.co.uk**](http://www.aquacure.co.uk)

**sales@aquacure.co.uk**