

**EcoAqua AQ35 Style (Instanta) Cartridge**

Code: EWF8005A



Fits the following filters:

Insinkerator® F-601, Instanta® AQ35.

**Operating Specifications:**

Minimum operating temperature 0.6°C/33°F

Maximum operating temperature 38°C/100°F

Min. working pressure 140 kPa/20 psi

Max. working pressure 827 kPa/120 psi

Rated capacity 13,250 litres/2,900 gallons

Flow rate 3.8 lpm/1 gpm





*Distributed by:*

**Aqua Cure Ltd,**

**Aqua Cure House, Hall Street,**

**Southport, PR9 0SE.**

**Tel: 01704 516916**

[**www.aquacure.co.uk**](http://www.aquacure.co.uk)

**sales@aquacure.co.uk**